3.1.4 WATER BALLAST SYSTEM

The ballast pump to be operated in accordance with IMO.3.4.5. The BWTS to be TECHCROSS, direct-electronic type.

3.1.3 REMOTE VALVE CONTROL SYSTEM

Remote valve for cargo valve to be operated remotely.

The drain plug for remote valve to be provided

3.1.5 BIGLE SYSTEM

Bilge on weather deck to be overboard via bilge pump in E/R.