3.1.3 REMOTE VALVE CONTROL SYSTEM

Remote valve for cargo valve to be operated remotely and manually by portable hand

pump. The additional hand pump to be supplied by Buyer.

3.1.4 WATER BALLAST SYSTEM

The ballast pump to be operated in accordance with IMO.3.4.5